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	Assessor
	Water Lane URC
	Date
	12.10.26

	Description
	Use of Electrical Equipment
	Review period
	12 months


	Task
	Hazard
	Risk
	Persons at risk
	Risk
Level 
(L x C)
	Control measures
	Residual Risk Level
(L x C)
	Action by
	Date to be completed

	Changing light bulbs and lamps

Re-wiring plugs
	Electric shock
	Death, burns
	Maintenance staff, hirers, church members and visitors
	4 x 5 =20
	· Only authorised persons to undertake electrical work.
· Authorised persons to be competent.
· Lights to be isolated (switched off) from any power sources. 
· Isolation switches ‘locked off’ and/or to be signed indicating persons working on the system. 
	2 x 5 = 10
	Church Elders
	Immediately

	Over-loading
plug sockets,
trailing extensions and ‘block’ adaptors

	Fire
	Death, 
burns,
asphyxia
	Maintenance staff, hirers, church members and visitors
	4 x 5 = 20
	· Check before using equipment for the following danger signs:
· blackness or scorch marks around a socket or plug, or on an appliance,
· damaged or frayed leads,
· coloured wire inside leads showing at the plug or anywhere else,
· melted plastic on appliance casings or leads.

· Whilst the appliance is being used:
· a smell of hot plastic or 
burning near an appliance or socket,
· sparks or smoke coming from a plug or appliance,
- fuses that blow or circuit-breakers that operate for no obvious reason.
	2 x 5 = 10
	All equipment users
	Ongoing

	Damaged wiring or plugs
	Fire, electric shock
	Death, 
burns,
asphyxia
	Maintenance staff, hirers, church members and visitors
	4 x 5 = 20
	· Portable Appliance Testing to be carried out at regular intervals in accordance with H&S Policy.
· Fixed Electrical Wiring Test to be carried out at least every five years.
	2 x 5 = 10
	Church Elders
	Ongoing

	Major electrical works
	Fire, electric shock
	Death, 
burns,
asphyxia
	Maintenance staff, hires, church members and visitors
	3 x 5 = 15
	· Only suitably qualified electricians to undertake such work. Competencies to be checked and details recorded. 
· All work to be certified on completion. 
	2 x 5 = 10
	Church Elders
	Ongoing

	Use of electrical equipment
(e.g. grass cutters, strimmer, vacuum cleaners, floor cleaners)
	Electric shock
	Death, 
burns,
asphyxia
	Maintenance staff, hirers, church members and visitors
	4 x 5 = 20
	· Equipment to be visually checked prior to use by operator.
· RCDs to be used on any equipment being operated in the outside or a damp environment.
· Portable equipment to be regularly tested by a competent person.
· Blockages or jams to be dealt with when the power has been switched off and appliance has been unplugged from the power source.
· Replace 230v AC equipment where possibly with battery operated cordless appliances. 
	2 x 5 = 10
	Church Elders
	Ongoing


	Name and position
	A Booth - Elder
	Signature
	
	Date completed
	12.10.26
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