[image: ]		RISK ASSESSMENT
	Assessor
	Water Lane URC
	Date
	12.10.26

	Description
	Working with Asbestos – Note that during major refurbishment works carried out in 2025 all roof and floor voids and the cellar were examined for asbestos during the works along with consultation of the 2025 asbestos survey. No asbestos containing materials were discovered on the site. 
	Review period
	12 months


	Task
	Hazard
	Risk
	Persons at risk
	Risk
Level 
(L x C)
	Control measures
	Residual Risk Level
(L x C)
	Action by
	Date completed

	Removal of thermal lagging / decoration of structural walls / partitions which may be cut or broken, or are allowed to deteriorate and break down.
	Inhalation of asbestos fibres where the asbestos-containing materials (ACMs) are disturbed.
	Death, lung disease

	Staff, hirers, visitors,
volunteers,
consultants, contractors
	5 x 5 = 25
	· Ensure that an Asbestos Survey has been carried out by a specialist company, and that appropriate control measures to prevent asbestos fibres from being released have been taken.
· Ensure that no building maintenance work or redecoration is carried out without reference to the Asbestos Register and survey report.
· Ensure that all staff are aware of the location of ACMs and awareness training is given to all staff who are likely to come into contact with ACMs. 
	2 x 5 =10
	Church Elders
	At the start of every new contract

	Drilling holes, minor repairs, any intrusion into the fabric of the building
	Inhalation of asbestos fibres where the asbestos-containing materials (ACMs) are disturbed.
	Death, lung disease

	Staff, hirers, visitors,
volunteers,
consultants, contractors
	5 x 5 = 25
	· ACMs to be identified by signage.
· Any person undertaking maintenance work to have completed Asbestos Awareness Training.
	3 x 5 =15
	Church Elders
	Immediately 


	Name and position
	A Booth - Elder
	Signature
	
	Date completed
	12.10.26
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