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	Assessor
	Water Lane URC
	Date
	12.10.26

	Description
	Slips, trips and falls
	Review period
	12 months


	Task
	Hazard
	Risk
	Persons at risk
	Risk
Level 
(L x C)
	Control measures
	Residual Risk Level
(L x C)
	Action by
	Date to be completed

	Walking on / across floors / ground.
	Wet floors and spillages.
	Slips, trips and falls, broken bones.
	Staff, hirers, church members, visitors and contractors
	4 x 4 = 16
	· Provision of non-slip floors where appropriate. 
· Ensure spillages are attended to immediately.
	 1 x 4 = 4
	Church Elders
	Immediately 

	Walking on / across floors / ground.
	Uneven or poor floor surfaces / changes in height of flooring.
	Slips, trips and falls, broken bones.
	Staff, hirers, church members, visitors and contractors
	4 x 4 = 16
	· Uneven flooring indicated with a warning sign.
· Change of height in flooring indicated with a warning sign.
· Maintenance of flooring kept to a high standard and repaired when broken
	 1 x 4 = 4
	Church Elders
	Immediately

	Walking on / across floors / ground.
	Obstructions located in thoroughfare.
	Slips, trips and falls, broken bones.
	Staff, hirers, church members, visitors and contractors
	4 x 4 = 16
	· Train staff and church members to place and store objects away from the thoroughfare.
· Good housekeeping to be maintained at all times.
· Refuse to be removed regularly to prevent build up.
· Bins to be provided at strategic points to ensure minimal waste deposited on floors. 
	 1 x 4 = 4
	Church Elders
	Immediately

	Walking on / across floors / ground.
	Trailing cables.

	Slips, trips and falls, broken bones.
	Staff, hirers, church members, visitors and contractors
	4 x 4 = 16
	· Tying in of electrical cables and provision of trunking for permanent cables such as computer leads and peripheries
	 1 x 4 = 4
	Church Elders
	Immediately


	Walking on / across floors / ground.
	Poor lighting.
	Slips, trips and falls, broken bones.
	Staff, hirers, church members, visitors and contractors
	4 x 4 = 16
	· Permanent lighting needs to provide a minimum level of lux to sustain safe working conditions.
· Where this is not possible, additional temporary lighting should be provided.
	 1 x 4 = 4
	Church Elders
	Immediately


	Walking on / across floors / ground.
	Adverse weather conditions.
	Slips, trips and falls, broken bones.
	Staff, hirers, church members, visitors and contractors
	4 x 4 = 16
	· Provision of non-slip floors where appropriate.
· Ensure collecting rainwater / snow is attended to immediately.
· Wear non-slip shoes where appropriate.
· Lighting needs to provide a level of lux to sustain safe working conditions - or additional lighting should be provided.
	 1 x 4 = 4
	Church Elders
	Immediately



	Name and position
	A Booth - Elder
	Signature
	
	Date completed
	12.10.26
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