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	Assessor
	Water Lane URC
	Date
	12.10.26

	Description
	Use of Audio Visual Equipment
	Review period
	12 months


	Task
	Hazard
	Risk
	Persons at risk
	Risk
Level 
(L x C)
	Control measures
	Residual Risk Level
(L x C)
	Action by
	Date to be completed

	Powering equipment on stage or at the front of the church
	Electric shock, fire
	Death, burns, asphyxia
	Ministers, 
worship leaders,
musicians, hirers, church members, 
visitors
	4 x 5 = 20
	· All electrical equipment (including personal equipment) to be Portable Appliance Tested at regular intervals (every 12 months).
· No ‘daisy chaining’ of trailing extensions.
· All extensions to be fully uncoiled to prevent over- heating.
· Sockets to be checked to prevent overloading.
· RCDs to be used on instruments connected via cables to powered units (e.g. guitars).
· CO2 fire extinguisher to be within easy access of stage users.
· All electrical equipment to be switched off when not in use or unattended.
	2 x 5 = 10
	Church Elders
	Ongoing

	Use of a sound desk
	Electric shock, fire
	Death, burns, asphyxia
	AV operators, hirers, cleaners
	4 x 5 = 20
	· Power cables to be secured in conduit or with cable ties.
· Equipment (desk, computer, etc.) to be appliance tested at regular intervals.
· No drinks or food to be consumed near the equipment.
· Operators to be competent to use equipment.
· Only authorised persons in the sound desk area.
· CO2 fire extinguisher to be readily available for desk operators.
	2 x 5 = 10
	Church Elders
	Ongoing

	Projector and screen
	Electric shock, fire, slips and trips, falling objects
	Death, burns, asphyxia, bruises, cuts, concussion
	Ministers, 
worship leaders,
musicians, hirers, church members, 
visitors
	4 x 5 = 20
	· Power cables secured in conduit or with cable ties to prevent damage or trips.
· Projector located away from combustible materials to reduce fire.
· Projector secured with wire cable to prevent falling.
· Screen secured to wall and securing mounts checked periodically.
· Projector and electric screen to be Portable Appliance Tested at regular intervals.
	2 x 5 = 10
	Church Elders
	Ongoing

	Speaker sound
	Excessive noise
	Hearing disorders 
	Ministers, 
worship leaders,
musicians, hirers, church members, 
visitors
	4 x 3 = 12
	· Main volume control to be through the sound desk.
· Persons are not to be positioned in front of any speakers for prolonged periods of time.
	2 x 3 = 6
	Church Elders
	Ongoing


	Name and position
	A Booth - Elder
	Signature
	
	Date completed
	12.10.26
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